[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: [FEMM] lua addmaterial() parameters

- To: FEMM mailing list <femm@list.foster-miller.net>
- Subject: Re: [FEMM] lua addmaterial() parameters
- From: David Meeker <dmeeker@ieee.org>
- Date: Wed, 28 Apr 2004 09:37:20 -0400
- In-reply-to: <OF414D47E6.00C0E02F-ON85256E83.005F99E0-85256E83.006033D1@checkpt.com>
- List-archive: <http://femm.foster-miller.net/pipermail/femm>
- List-help: <mailto:femm-request@list.foster-miller.net?subject=help>
- List-id: FEMM mailing list <femm.list.foster-miller.net>
- List-post: <mailto:femm@list.foster-miller.net>
- List-subscribe: <http://femm.foster-miller.net/mailman/listinfo/femm>, <mailto:femm-request@list.foster-miller.net?subject=subscribe>
- List-unsubscribe: <http://femm.foster-miller.net/mailman/listinfo/femm>, <mailto:femm-request@list.foster-miller.net?subject=unsubscribe>
- References: <OF414D47E6.00C0E02F-ON85256E83.005F99E0-85256E83.006033D1@checkpt.com>
- Reply-to: FEMM mailing list <femm@list.foster-miller.net>
- User-agent: Mozilla/5.0 (Windows; U; Windows NT 5.1; en-US; rv:1.6) Gecko/20040113 MultiZilla/1.6.0.0e

`RONALD.SALESKY@checkpt.com wrote:`

> `The lua addmaterial( ) function has a 'theta_h' parameter which allows defining hysteresis lag angle which is good for modelling isotropic materials, but how does one specify the angle for anisotropic materials in lua, which can be done from within the FEMM editor when defining a material?`

`
I forgot to update the documentation in v3.3 for this command. The documentation says that the command takes 11 parameters. If you enter 2 more parameters, they are used as the theta_hx and theta_hy parameters like those in the material definition dialog. If only 11 parameters are specified, it just takes the value of theta_h for theta_hx and theta_hy. The command appears to be properly documented in v4.`
`Dave.`

- References:
  - [FEMM] lua addmaterial() parameters
    - From: RONALD.SALESKY@checkpt.com

- Prev by Date: [FEMM] lua addmaterial() parameters
- Next by Date: Re: [FEMM] Femm 4.0 Post Processor scripting
- Previous by thread: [FEMM] lua addmaterial() parameters
- Next by thread: [FEMM] getpointvalues use
- Index(es):
  - Date
  - Thread