[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: [femm] Re: Can femm model this?

- To: femm@yahoogroups.com
- Subject: Re: [femm] Re: Can femm model this?
- From: "H.Hasper" <h.Hasper@fwn.rug.nl>
- Date: Thu, 31 Jul 2003 10:45:19 +0200
- In-reply-to: <bg9qm2+ni91@eGroups.com>

`Hi wigstonmagna,`
`your problem can easely be solved by FEMLAB multiphysics FEM software.
The links: www.femlab.com
and
www.mathworks.com`
`Hendrik Hasper`

    On Thu, 31 Jul 2003 01:16:50 -0000
    "" <andrew_ppp@hotmail.com> wrote:

> `wigstonmagna wrote:
> I want to simulate a coil placed between two flat parallel metal plates, with the coil's long axis parallel to the plates. I want to electrically connect the inductance in parallel with the capacitor (the plates) and drive the assembly at AC.
> Can this be constructed?
> -Andrew`
> `David replied:
> Problems that FEMM can simulate have to be either axially symmetric (e.g. a solenoid, speaker driver, etc.) or approximated as planar (e.g. many types of motors). Although your coil may be axisymmetric, the entire arrangement isn't axisymmetric--you can't model it directly with FEMM.`
> `How about planar mode? Will a 2D slice work?`
> ``
> `------------------------ Yahoo! Groups Sponsor`
> ``
> `Your use of Yahoo! Groups is subject to http://docs.yahoo.com/info/terms/`

`
Dr. H. Hasper
Fysische Informatica Applied Computer Science
Rijksuniversiteit Groningen University of Groningen Nijenborgh 4
9747 AG Groningen The Netherlands
tel.: +.31.(0)50.3634745
fax.: +.31.(0)50.3636837
E-mail: h.hasper@phys.rug.nl`

- References:
  - Re: Can femm model this?
    - From: "wigstonmagna" <andrew_ppp@hotmail.com>

- Prev by Date: Re: Can femm model this?
- Next by Date: Problem with the unit of H
- Previous by thread: Re: Can femm model this?
- Next by thread: Re: Can femm model this?
- Index(es):
  - Date
  - Thread