[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: [femm] direction of magnitization

- To: femm@yahoogroups.com
- Subject: Re: [femm] direction of magnitization
- From: David Meeker <dmeeker@ieee.org>
- Date: Wed, 17 Apr 2002 14:04:14 -0400
- References: <000001c1e545$44f6e5a0$0200a8c0@DELL>
- User-agent: Mozilla/5.0 (Windows; U; Windows NT 5.0; en-US; rv:0.9.9) Gecko/20020311

`Brad Frustaglio wrote:`

> `I just started using feem 3.1 from 2.1.`

>     How do define the direction of magnetization for permanent magnets? If I
>     remember right, there was an input on the "Block Property" form in the
>     2.1 version.

> `Any help will be appreciated.`
> `Thanks,`
> `Brad Frustaglio`

`Since 2.1, the definition of the magnetization direction has been changed to a property that is assigned to individual block labels, in a similar fashion to the way that material properties are assigned to block labels.`
`Dave.`
``

- References:
  - direction of magnitization
    - From: "Brad Frustaglio" <bmfrusta@yahoo.com>

- Prev by Date: FEMM on Linux
- Next by Date: Lua questions
- Previous by thread: Re: direction of magnitization
- Next by thread: RE: [femm] Coil with multiple turns
- Index(es):
  - Date
  - Thread