[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# RE: [femm] Export X-Y field plot?

- To: "'femm@yahoogroups.com'" <femm@yahoogroups.com>
- Subject: RE: [femm] Export X-Y field plot?
- From: "Guy, James K" <james.k.guy@boeing.com>
- Date: Tue, 19 Nov 2002 16:15:40 -0700

    Thanks David! I got it...

    -----Original Message-----
    From: David Meeker [mailto:dmeeker@ieee.org]
    Sent: Tuesday, November 19, 2002 3:12 PM
    To: femm@yahoogroups.com
    Subject: Re: [femm] Export X-Y field plot?

    Guy, James K wrote:

    > David-
    >
    > On that same topic, Is the x-y plot nominally oriented at x=0, y=0 ? Do I
    > have to move my geometry such that the section under question is cut
    > by the
    > x-axis oriented at (0,0)?
    >
    > Thanks,
    >
    > Kevan

    Perhaps "X-Y plot" is a something of a misnomer--what the "X-Y plot"
    really represents is the plot of some user-specified quantity along an
    arbitrary user-defined contour. The x-y plot is not nominally oriented
    at x=y=0. You can start and end the contour at any points that you desire.

    When you then make a plot, the horizontal axis (or first column, if you
    are writing the info to disk) is a length in whatever units that you
    used when you drew the problem geometry. The horizontal axis always
    starts from zero, and this length represents the distance along the
    user-defined contour as measured from the starting point of the contour.

    Dave.
    --
    David Meeker
    email: dmeeker@ieee.org
    www: http://femm.berlios.de/dmeeker

    Your use of Yahoo! Groups is subject to http://docs.yahoo.com/info/terms/

- Prev by Date: Re: [femm] Export X-Y field plot?
- Next by Date: Induction motor no load test
- Previous by thread: Re: [femm] Export X-Y field plot?
- Next by thread: Induction motor no load test
- Index(es):
  - Date
  - Thread