[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: Rif: [femm] Problem with triangle on femm3.3

- To: femm@yahoogroups.com
- Subject: Re: Rif: [femm] Problem with triangle on femm3.3
- From: Tsarafidy RAMINOSOA <tsarafidy@yahoo.fr>
- Date: Thu, 25 Sep 2003 18:22:16 +0200 (CEST)
- In-reply-to: <OF0EA881E3.F5DF83C8-ONC1256DAC.0056DE2C@sogagroup.com>

Cool,
Thanks a lot ! It works well now.
Yes, it's better to let triangle choose automatically the mesh size rather than giving non realistic value.
Thanks for giving me an idea of the different blocks ' mesh size that I should use.
Tsarafidy.
giovanni.bortolan@sogagroup.com wrote:

> `
> Try the attached file.
> You where right thin angles were the problem.
> I have removed al couple of layers at each side of the rotor and changed
> air gap's minimum segment to 1deg. I also changed many blocks' sizes.
> (See attached file: sinc_reluc.fem)
> _______________________________
> ing. G.Bortolan
> Sincro srl
> via Tezze, 3 loc. Cereda
> 36073 Cornedo Vicentino (VI)
> ITALY
> Tel: (++39) 0445 450 500
> Fax: (++39) 0445 446 190
> e-mail: Giovanni.Bortolan@sogagroup.com
> tecnico.sincro@sogagroup.com
> http://www.sogagroup.com
> REA 194515/VI
> Reg. Imp. 20968/VI 116
> P.IVA 01925820241
> Tsarafidy
> RAMINOSOA Per: femm@yahoogroups.com
> <tsarafidy@yahoo Cc:
> .fr> Oggetto: [femm] Problem with triangle on femm3.3
> 25/09/2003 12:21
> Per favore,
> rispondere a
> femm
> Hi all,
> I attached a model of axially laminated synchronous reluctance machine.
> I tried to run it on femm3.3 but triangle always crashes. I think the cause
> is the presence of very thin angles at the rotor side laminations.
> Do anyone already had this kind of problem? How did he proceed to solve it
> ?
> If this was already pointed out in this forum, it would be kind to post me
> the messages references.
> Any other comment will be welcome.
> Thanks in advance,
> Regards,
> Tsarafidy
> `
> `Your use of Yahoo! Groups is subject to the Yahoo! Terms of Service.`
> > ATTACHMENT part 2 application/octet-stream name=sinc_reluc.fem

Do You Yahoo!? -- Une adresse @yahoo.fr gratuite et en français !
Testez le nouveau Yahoo! Mail

- References:
  - Rif: [femm] Problem with triangle on femm3.3
    - From: giovanni.bortolan@sogagroup.com

- Prev by Date: Re: some proposals for future developments
- Next by Date: Two phase induction motor
- Previous by thread: Rif: [femm] Problem with triangle on femm3.3
- Next by thread: Two phase induction motor
- Index(es):
  - Date
  - Thread