[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: Saving the "meshed" model in FEMM as a *.DXF file

- To: femm@yahoogroups.com
- Subject: Re: Saving the "meshed" model in FEMM as a *.DXF file
- From: "David Meeker" <dmeeker@ieee.org>
- Date: Tue, 13 May 2003 21:59:12 -0000
- In-reply-to: <b9q9t8+cib2@eGroups.com>
- User-agent: eGroups-EW/0.82

    --- In femm@yahoogroups.com, "israelkk2001" <tsiporak@h...> wrote:
    > Dear David:
    >
    > It can be very usefull for me if there will an option in FEMM to
    > save (export) the model drawing as a *.DXF file including the mesh
    > lines as an option too (not just the outside lines of the models). I
    > hope it can be done.
    >
    > Sincerely,
    >
    >
    > Israel Kehaty

    Check out:
    http://groups.yahoo.com/group/femm/files/dxfmesh.zip
    This is a command-line utility for chewing up the *.node and *.edge
    file associated with a problem and spitting out a *.dxf file from that
    info.

    For example, if your geometry was stored in file.fem, the command line
    to run the program would be:

    dxfmesh file > filemesh.dxf

    where the output would be piped to the file filemesh.dxf
    --
    David Meeker
    http://femm.berlios.de/dmeeker

- References:
  - Saving the "meshed" model in FEMM as a *.DXF file
    - From: "israelkk2001" <tsiporak@hotmail.com>

- Prev by Date: BH curve of steel-37 (?)
- Next by Date: back-emf calculation in dc motor
- Previous by thread: Saving the "meshed" model in FEMM as a *.DXF file
- Next by thread: fkn.exe
- Index(es):
  - Date
  - Thread