[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# [femm] Re: part motor stator modeling???

- To: femm@egroups.com
- Subject: [femm] Re: part motor stator modeling???
- From: Dcm3c@aol.com
- Date: Tue, 28 Mar 2000 09:43:51 EST
- Delivered-to: listsaver-of-femm@egroups.com
- Delivered-to: listsaver-egroups-femm@egroups.com
- List-archive: <http://www.egroups.com/group/femm/>
- List-help: <http://www.egroups.com/group/femm/info.html>, <mailto:femm-help@egroups.com>
- List-unsubscribe: <mailto:femm-unsubscribe@egroups.com>
- Mailing-list: contact femm-owner@egroups.com
- Reply-to: femm@egroups.com

    In a message dated 3/23/00 2:22:50 AM Eastern Standard Time,
    pvallian@central.ntua.gr writes:

    > i have just finished modeling a 400kw/6kv induction motor/ complete
    > stator. Was it possible to model only a pole?
    > If yes, how do you insert the limit conditions (periodic / aperiodic)
    > of potential in the borders of the model??

    The program currently can't do periodic boundary conditions--you have to
    model the whole machine, unless things are symmetric enough to apply A=0 or
    dA/dn=0 boundary conditions to get the symmetry.

    Dave.

- Prev by Date: [femm] Re: part motor stator modeling???
- Next by Date: Re: [femm] Adress
- Previous by thread: [femm] Re: part motor stator modeling???
- Next by thread: Re: [femm] Adress
- Index(es):
  - Date
  - Thread