[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: inductance - parallel strips

- To: femm@yahoogroups.com
- Subject: Re: inductance - parallel strips
- From: tborzic@yahoo.com
- Date: Mon, 19 Nov 2001 18:10:50 -0000
- In-reply-to: <F12ZHLtGw9A5BN36wPd0000b589@hotmail.com>
- User-agent: eGroups-EW/0.82

    > To Dear Tomislav:
    >
    > How are you? Did you get inductance, L(femm)=1.1517 e-6 H/m, with
    your
    > FEM model? I did not. At a glance, there is no space, left of left
    conductor
    > and right of right conductor, and top and bottom too. In other
    words, there
    > is no room for filed to develop fully. Or, the text file attached
    was
    > corrupted in the delivery via e-mail ?
    >
    > Thanks
    > Sincerely,
    > SE-HO YOU

    well, in "my" model, I just marked conductors (areas) and callculated
    A.J integral, which divided by i^2 (1A) gives 1.15 e-6 H/m.
    i didn't defined any boundaries because femm takes such boundary as
    dA/dn = 0 boundary. so, point was to keep flux from closing trough
    conductors.
    Tomislav

- References:
  - Re: [femm] Re: inductance - parallel strips
    - From: "you se-ho" <sxy28@hotmail.com>

- Prev by Date: Re: [femm] Inductance by means of his definition
- Next by Date: Re: induction machine inductance calculations
- Previous by thread: Re: [femm] Re: inductance - parallel strips
- Next by thread: Re: [femm] Re: inductance - parallel strips
- Index(es):
  - Date
  - Thread