[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Other improvements

- To: femm@yahoogroups.com
- Subject: Other improvements
- From: Dave Squires <djsquires@plix.com>
- Date: Thu, 24 Apr 2003 10:17:07 -0700
- References: <b88svr+gnka@eGroups.com>
- User-agent: Mozilla/5.0 (Windows; U; Win 9x 4.90; en-US; rv:1.0.1) Gecko/20020823 Netscape/7.0

`David,`
`As long as we are on the topic of improvements....`

    How about looking into some way to handle tapewound
    laminations? This would mean say a tapewound toroid
    or rectangular core of something like Si steel or Metglas.
    At present FEMM allows only specifying an orthogonal
    lamination direction in X or Y directions or "in-plane".
    This means that on-screen you would be looking
    at the laminations on edge and they would follow
    the shape contour and not be restricted only to
    X or Y directions. I know this would be a big
    programming headache, but it would help a lot for
    some of us to get more realistic results for these
    kinds of structures.

    Regards,
    Dave Squires

- References:
  - Re: Vector plots + "zoomier"
    - From: "David Meeker" <dmeeker@ieee.org>

- Prev by Date: Re: Vector plots + "zoomier"
- Next by Date: AC and DC currents in FEMM? Is this possible?
- Previous by thread: Re: Vector plots + "zoomier"
- Next by thread: LIM....please help me^^
- Index(es):
  - Date
  - Thread