[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# [FEMM] How to freeze the reluctivities in each element?

- To: femm@list.foster-miller.net
- Subject: [FEMM] How to freeze the reluctivities in each element?
- From: Ramdane LATEB <ramdane.lateb@ensem.inpl-nancy.fr>
- Date: Wed, 17 Dec 2003 17:21:34 +0100
- List-archive: <http://femm.foster-miller.net/pipermail/femm>
- List-help: <mailto:femm-request@list.foster-miller.net?subject=help>
- List-id: FEMM mailing list <femm.list.foster-miller.net>
- List-post: <mailto:femm@list.foster-miller.net>
- List-subscribe: <http://femm.foster-miller.net/mailman/listinfo/femm>, <mailto:femm-request@list.foster-miller.net?subject=subscribe>
- List-unsubscribe: <http://femm.foster-miller.net/mailman/listinfo/femm>, <mailto:femm-request@list.foster-miller.net?subject=unsubscribe>
- Reply-to: FEMM mailing list <femm@list.foster-miller.net>

`Hello,
I'm simulating an induction machine under a non linear field solution with femm and through lua language, I need to calculate all parameters of the machine. The idea is to determine all the parameters of the equivalent circuit of a specific slip frequency. For this purpose I need to freeze the reluctivities of each element found from the latest non linear field solutions and perform a linear FE calculation at synchronous speed with slip=0 (for the details see Ping Zhou."Finite Element Analysis of Induction Motors Based on Computing Detailed Equivalent Circuit Parameters, IEEE Trans. On Magn. Vol. 34; N°.5., Sept 1998". The problem is that I don't know how to get the reluctivities of each element through lua (in femm).
Any idea is welcome`
``

- Follow-Ups:
  - Re: [FEMM] How to freeze the reluctivities in each element?
    - From: David Meeker <dmeeker@foster-miller.com>

- Prev by Date: [FEMM] Two phase induction motor
- Next by Date: Re: [FEMM] How to freeze the reluctivities in each element?
- Previous by thread: [FEMM] [Fwd: Book on Variable Reluctance Machines]
- Next by thread: Re: [FEMM] How to freeze the reluctivities in each element?
- Index(es):
  - Date
  - Thread