[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: [femm] Bug in move function

- To: femm@yahoogroups.com
- Subject: Re: [femm] Bug in move function
- From: "David Meeker <dcm3c@earthlink.net>" <dcm3c@earthlink.net>
- Date: Mon, 09 Dec 2002 14:24:45 -0000
- In-reply-to: <OF905E011E.51A637AB-ONC1256C8A.003A8250@sogagroup.com>
- User-agent: eGroups-EW/0.82

    --- In femm@yahoogroups.com, giovanni.bortolan@s... wrote:
    >
    > Thank you David,
    > it was exactly as you supposed. That is a possible problem
    > working with snap to grid
    >
    > Another small thing:
    > When I mirror a geometry the magnetization direction of
    > magnets is not mirrored, It seems to be not consistent with
    > rotate operation.

    Ok, I can readily duplicate this. Like you say, the magnet direction
    should be changed so that it is mirrored as well. Thanks a lot for
    pointing it out--I'll fix this in the next program update.

    Dave.

- References:
  - Rif: Re: [femm] Bug in move function
    - From: giovanni.bortolan@sogagroup.com

- Prev by Date: Re: [femm] Bearing currents and faraday cage
- Next by Date: 'block' and 'group' confussion
- Previous by thread: Rif: Re: [femm] Bug in move function
- Next by thread: Re: [femm] Bearing currents and faraday cage
- Index(es):
  - Date
  - Thread