[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: [femm] Problem in lua script with probdef()

- To: femm@yahoogroups.com
- Subject: Re: [femm] Problem in lua script with probdef()
- From: David Meeker <dmeeker@ieee.org>
- Date: Mon, 28 Apr 2003 17:35:23 -0400
- In-reply-to: <000601c30d44$186ade60$14715142@robertmacy>
- References: <b8drsh+b1e0@eGroups.com> <000601c30d44$186ade60$14715142@robertmacy>
- User-agent: Mozilla/5.0 (Windows; U; Windows NT 5.1; en-US; rv:1.3; MultiZilla v1.4.0.3H) Gecko/20030312

`Robert Macy wrote:`

>     Ran across problem trying to run lua script when using the probdef()
>     statement.
>     The manual says you can ask for a variety of units.

>     My problem was in thousandths of an inch so I used "mils" The program
>     wouldn't run if that is used.

>     I tried
>     Mils MILS mil mls all to no avail,
>     but "mills" worked.

> `- Robert -`

`Thanks for pointing this out--I'll make sure that "mils" works right when I post the next minor update of the program. Note that the same bug also is mirrored in the electrostatics version, beladraw--I'll get that one in the next minor update, too.`
`Dave.`

    --
    David Meeker
    dmeeker@ieee.org
    http://femm.berlios.de/dmeeker

``

- Follow-Ups:
  - Calculating rotor-bar inductance in a SCI motor
    - From: "Tielman Slabbert" <tielman01@telkomsa.net>

- References:
  - AC and DC currents in FEMM? Is this possible?
    - From: "daniel_handloser" <daniel_handloser@yahoo.de>
  - Problem in lua script with probdef()
    - From: "Robert Macy" <macy@california.com>

- Prev by Date: Re: [femm] AC and DC currents in FEMM? Is this possible?
- Next by Date: Calculating rotor-bar inductance in a SCI motor
- Previous by thread: Problem in lua script with probdef()
- Next by thread: Calculating rotor-bar inductance in a SCI motor
- Index(es):
  - Date
  - Thread