[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# [FEMM] Need BH curves for deposited Permalloy

- To: femm@list.foster-miller.net
- Subject: [FEMM] Need BH curves for deposited Permalloy
- From: "robert Macy" <macy@california.com>
- Date: Fri, 31 Oct 2003 14:33:05 -0800
- In-reply-to: <893B4A5E16B1D611934A00D0B7278CDC47A2@cad-exchange-1.engineering.linear.com>
- List-archive: <http://femm.foster-miller.net/pipermail/femm>
- List-help: <mailto:femm-request@list.foster-miller.net?subject=help>
- List-id: Finite Element Method Magnetics mailing list <femm.list.foster-miller.net>
- List-post: <mailto:femm@list.foster-miller.net>
- List-subscribe: <http://femm.foster-miller.net/mailman/listinfo/femm>, <mailto:femm-request@list.foster-miller.net?subject=subscribe>
- List-unsubscribe: <http://femm.foster-miller.net/mailman/listinfo/femm>, <mailto:femm-request@list.foster-miller.net?subject=unsubscribe>
- Reply-to: Finite Element Method Magnetics mailing list <femm@list.foster-miller.net>

    Hi group,

    Does anyone have BH curves for deposited permalloy
    material?  The material is 4-79 Permalloy, which stands for
    79% Ni, 17% Fe, and 4% Mo.  When deposited, its thickness
    is in the 7 to 15 micron range.

    I know it can be worked on after deposition to controllably
    change its characteristics, but right now I have almost
    nothing as a starting point.

    Alas, my Google searches have yielded the normal spate of
    ads, expired web pages, and unrelated articles.

                      - Robert -

- Prev by Date: Re: [FEMM] Tape wound core modeling
- Next by Date: [FEMM] BH curves for 52100 hardened bearing steel
- Previous by thread: [FEMM] Merry Christmas to David !!!
- Next by thread: Re: [FEMM] Need BH curves for deposited Permalloy
- Index(es):
  - Date
  - Thread