[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Negative Group Numbers

- To: femm@yahoogroups.com
- Subject: Negative Group Numbers
- From: Joe Riel <joer@k-online.com>
- Date: Tue, 21 May 2002 15:43:14 -0700
- In-reply-to: <3CE9BF99.5090009@ieee.org>

    It would be convenient if negative group numbers were allowed.
    FEMM doesn't balk when they are entered; however,
    the groupselectblock command doesn't select any blocks with negative group numbers.

    The reason that this would be convenient is that
    it simplifies the task of assigning directions to currents in a planar analysis.
    For example, I would like to assign group numbers of +n and -n to the two ends
    of the conductor(s) that make up winding n.

    Joe Riel

- References:
  - Re: [femm] problem with convergence
    - From: David Meeker <dmeeker@ieee.org>

- Prev by Date: Pseudo 3D
- Next by Date: Re: [femm] Re: Torque calculation (2)
- Previous by thread: Re: [femm] problem with convergence
- Next by thread: Force on a conductor?
- Index(es):
  - Date
  - Thread