[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: [FEMM] Another suggestion for the next version?

- To: Finite Element Method Magnetics mailing list <femm@list.foster-miller.net>
- Subject: Re: [FEMM] Another suggestion for the next version?
- From: David Meeker <dmeeker@ieee.org>
- Date: Fri, 14 Nov 2003 12:54:13 -0500
- In-reply-to: <3FB3A470.1000909@aon.at>
- List-archive: <http://femm.foster-miller.net/pipermail/femm>
- List-help: <mailto:femm-request@list.foster-miller.net?subject=help>
- List-id: Finite Element Method Magnetics mailing list <femm.list.foster-miller.net>
- List-post: <mailto:femm@list.foster-miller.net>
- List-subscribe: <http://femm.foster-miller.net/mailman/listinfo/femm>, <mailto:femm-request@list.foster-miller.net?subject=subscribe>
- List-unsubscribe: <http://femm.foster-miller.net/mailman/listinfo/femm>, <mailto:femm-request@list.foster-miller.net?subject=unsubscribe>
- References: <3FB3A470.1000909@aon.at>
- Reply-to: Finite Element Method Magnetics mailing list <femm@list.foster-miller.net>
- User-agent: Mozilla/5.0 (Windows; U; Windows NT 5.1; en-US; rv:1.5; MultiZilla v1.5.0.2d) Gecko/20031007

`Alex Thaler wrote:`

> `I do a lot of permanent magent sync. machine modelling and i saw throughout the point properties in FemmView, that the H- Vektor in permanent magnets is not corrected for the Hc- value (vector?). So the summ of Hi*li is not zero when we go around a fluxline. Of course if someone knows, there is no problem in interpreting the right value of H in the magnets.`
> `I think David knows about that, but i want to know if i am right in reading the View-plot!`
> `Regards`
> `Alex`

`
FEMM reports H the way that it does because I like to think about magnets as I'd described previously in: http://femm.foster-miller.net/pipermail/femm/attachments/20010625/52c56cc3/attachment.html`
`However, I'm tired of explaining this, and everyone's probably tired of hearing about it. I've put a new preference in my development version of the program so that if the preference is turned on, the H reported inside permanent magnets will be the H as currently reported with Hc subtracted off of it.`
`Dave`

- Follow-Ups:
  - Re: [FEMM] Another suggestion for the next version?
    - From: Alex Thaler <alex.thaler@aon.at>

- References:
  - [FEMM] Another suggestion for the next version?
    - From: Alex Thaler <alex.thaler@aon.at>

- Prev by Date: [FEMM] 3-D interface
- Next by Date: Re: [FEMM] Another suggestion for the next version?
- Previous by thread: [FEMM] Another suggestion for the next version?
- Next by thread: Re: [FEMM] Another suggestion for the next version?
- Index(es):
  - Date
  - Thread