[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: [femm] 'block' and 'group' confussion

- To: femm@yahoogroups.com
- Subject: Re: [femm] 'block' and 'group' confussion
- From: Jiri Vecerka <vecerkaj@yahoo.com>
- Date: Tue, 10 Dec 2002 00:23:08 -0800 (PST)
- In-reply-to: <at3524+fp2h@eGroups.com>

    --- "Penquista66 <jtapia@die.udec.cl>"
    <jtapia@die.udec.cl> wrote:
    > Could anyone clarify me the difference between
    > 'block' and 'group'?.

    Block defines block type (material), mesh size, ciruit
    and assigmnent to a group for an area in which the
    block is located.
    Group is a feature you can use, if you want select on
    one click more entities. You can asign to one group
    nodes, line, arc, blocks. The group you will find
    usefull for example if you need to rotate a rotor of a
    motor. ALl entities of the rotor you will assign to
    one group (number diferent from 0), after that you
    choose group operation and after that simply click on
    a entity of the rotor. You will see, all entities of
    the rotor will be selected :-)).

    Jiri Vecerka

    __________________________________________________
    Do you Yahoo!?
    Yahoo! Mail Plus - Powerful. Affordable. Sign up now.
    http://mailplus.yahoo.com

- Follow-Ups:
  - RE: [femm] 'block' and 'group' confussion
    - From: "Juan Tapia" <jtapia@die.udec.cl>

- References:
  - 'block' and 'group' confussion
    - From: "Penquista66 <jtapia@die.udec.cl>" <jtapia@die.udec.cl>

- Prev by Date: Lua command for select segments over a region.
- Next by Date: Re: [femm] Lua command for select segments over a region.
- Previous by thread: 'block' and 'group' confussion
- Next by thread: RE: [femm] 'block' and 'group' confussion
- Index(es):
  - Date
  - Thread