[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# [FEMM] Another suggestion for the next version?

- To: Finite Element Method Magnetics mailing list <femm@list.foster-miller.net>
- Subject: [FEMM] Another suggestion for the next version?
- From: Alex Thaler <alex.thaler@aon.at>
- Date: Thu, 13 Nov 2003 16:34:08 +0100
- List-archive: <http://femm.foster-miller.net/pipermail/femm>
- List-help: <mailto:femm-request@list.foster-miller.net?subject=help>
- List-id: Finite Element Method Magnetics mailing list <femm.list.foster-miller.net>
- List-post: <mailto:femm@list.foster-miller.net>
- List-subscribe: <http://femm.foster-miller.net/mailman/listinfo/femm>, <mailto:femm-request@list.foster-miller.net?subject=subscribe>
- List-unsubscribe: <http://femm.foster-miller.net/mailman/listinfo/femm>, <mailto:femm-request@list.foster-miller.net?subject=unsubscribe>
- Reply-to: Finite Element Method Magnetics mailing list <femm@list.foster-miller.net>
- User-agent: Mozilla/5.0 (Windows; U; Windows NT 5.1; en-US; rv:1.5) Gecko/20031007

`I do a lot of permanent magent sync. machine modelling and i saw throughout the point properties in FemmView, that the H- Vektor in permanent magnets is not corrected for the Hc- value (vector?). So the summ of Hi*li is not zero when we go around a fluxline. Of course if someone knows, there is no problem in interpreting the right value of H in the magnets.`
`I think David knows about that, but i want to know if i am right in reading the View-plot!`
`Regards`
`Alex`

- Follow-Ups:
  - Re: [FEMM] Another suggestion for the next version?
    - From: David Meeker <dmeeker@ieee.org>

- Prev by Date: [FEMM] BH curves for 52100 hardened bearing steel
- Next by Date: [FEMM] 3-D interface
- Previous by thread: [FEMM] BH curves for 52100 hardened bearing steel
- Next by thread: Re: [FEMM] Another suggestion for the next version?
- Index(es):
  - Date
  - Thread