[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Problem in lua script with probdef()

- To: <femm@yahoogroups.com>
- Subject: Problem in lua script with probdef()
- From: "Robert Macy" <macy@california.com>
- Date: Sun, 27 Apr 2003 22:07:40 -0700
- Organization: AJM Electronics
- References: <b8drsh+b1e0@eGroups.com>
- Reply-to: "Robert Macy" <macy@california.com>

    Ran across problem trying to run lua script when using the probdef()
    statement.
    The manual says you can ask for a variety of units.

    My problem was in thousandths of an inch so I used "mils" The program
    wouldn't run if that is used.

    I tried
    Mils MILS mil mls all to no avail,
    but "mills" worked.

    - Robert -

- Follow-Ups:
  - Re: [femm] Problem in lua script with probdef()
    - From: David Meeker <dmeeker@ieee.org>

- References:
  - AC and DC currents in FEMM? Is this possible?
    - From: "daniel_handloser" <daniel_handloser@yahoo.de>

- Prev by Date: AC and DC currents in FEMM? Is this possible?
- Next by Date: Re: [femm] AC and DC currents in FEMM? Is this possible?
- Previous by thread: AC and DC currents in FEMM? Is this possible?
- Next by thread: Re: [femm] Problem in lua script with probdef()
- Index(es):
  - Date
  - Thread