[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Incorrect Field values returned by FEMM

- To: femm@yahoogroups.com
- Subject: Incorrect Field values returned by FEMM
- From: "cgn38nuc" <cgn38nuc@yahoo.com>
- Date: Thu, 06 Dec 2001 20:56:30 -0000
- User-agent: eGroups-EW/0.82

    I am using FEMM 3.1 to analysis a lifting magnet. The results as
    returned by the program indicate a maximum B value of 5.3 Tesla 4"
    from the working surface of the magnet. But, the saturation of steel
    only produces slighly more than 2 Tesla. I wasusing the B-H curve of
    1020 Steel in my formulation. What am I missing from my analysis.

    Thank you,
    Paul Sheridan

- Follow-Ups:
  - Re: [femm] Incorrect Field values returned by FEMM
    - From: David Meeker <dcm3c@earthlink.net>
  - Re: Incorrect Field values returned by FEMM
    - From: "vecerkaj" <vecerkaj@yahoo.com>

- Prev by Date: Re: [femm] Why femm sometimes never finised the calculation ?
- Next by Date: Re: Why femm sometimes never finised the calculation ?
- Previous by thread: Re: [femm] Re: Why femm sometimes never finised the calculation ?
- Next by thread: Re: [femm] Incorrect Field values returned by FEMM
- Index(es):
  - Date
  - Thread