[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: [femm] Default view settings

- To: femm@yahoogroups.com
- Subject: Re: [femm] Default view settings
- From: "Prem Kumar C" <prem@bhelrnd.co.in>
- Date: Sat, 09 Feb 2002 08:39:11 +0530
- References: <758E5D08839B9242B4514D01A2B4D591B539@dvrsql.dvrhome.com>

    Carl :
    It's very simple.
    In the Pre-processor(Editor) window select Edit/Preferences. You can set them all as per your choice. The THREE Check Boxes can be set to ON. Just Click OK thereon. Exit Editor. Once again open the Editor - you'll find
    the settings present.
    Likewise in the Post-processor(femm- viewer) in the Edit/ Preferences menu you'll find a similar table of Options. You can set them all to your liking. Click on OK. Close the window. The settings actuate on re-opening
    femm-view.
    Go on Carl .... Experiment with it ... !!
    Remember .... F in FEMM stands for fabulous ...!!

    C.Prem Kumar

    Carl Kopin wrote:

    > Dear Group
    >
    > does anyone know how to set grid size on an existing femm file that would stay permanently and not default to 10 or any other number every time I open this file? Similar problem with the result files (post-processor).
    >
    > Thanks,
    > Carl
    >
    >
    >
    >
    > Your use of Yahoo! Groups is subject to http://docs.yahoo.com/info/terms/

    begin:vcard
    n:Kumar;C.Prem Kumar
    tel;fax:+91 40 307 3820
    tel;home:+91 40 775 1195
    tel;work:+91 40 388 2347
    x-mozilla-html:FALSE
    org:Electromagnetics Group;BHEL Corp.R&D Division
    adr:;;Vikasnagar P.O,;Hyderabad;Andhra Pradesh;500 093;India
    version:2.1
    email;internet:prem@bhelrnd.co.in
    title:Deputy General Manager
    x-mozilla-cpt:;27744
    fn:C.Prem Kumar
    end:vcard

- References:
  - Default view settings
    - From: "Carl Kopin" <ckopin@davinciresearch.com>

- Prev by Date: Re: [femm] Triangulation!
- Next by Date: nonferrous electromagnets
- Previous by thread: Default view settings
- Next by thread: nonferrous electromagnets
- Index(es):
  - Date
  - Thread