[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: permanent magnet in harmonic analysis

- To: femm@yahoogroups.com
- Subject: Re: permanent magnet in harmonic analysis
- From: "dcm3c" <dcm3c@earthlink.net>
- Date: Thu, 10 Jan 2002 14:50:14 -0000
- In-reply-to: <20020109104133.86076.qmail@web21202.mail.yahoo.com>
- User-agent: eGroups-EW/0.82

    --- In femm@y..., E-J Borkent <eborkent@y...> wrote:
    > Hello,
    >
    > You told me that I could superimpose the results from
    > the static and the harmonic analysis. Is it possible
    > to export the data to a database or elsewhere in order
    > to be able to add the results easily.
    >
    > If I understand your answer well, it is not possible
    > to analyse the effect of an alternating current in my
    > coil in the field of a permanent magnet?
    >
    > I added my file to this e-mail. Thanks
    >
    > E-J Borkent

    Well, it just isn't possible to get both effects at the same time,
    because you can only analyze one frequency at a time. The magnet
    produces a DC field, and the coil an AC field.

    Anyhow, if you are interested in superimposing the fields manually, it
    is possible to dump data to disk, for example, off of a regularly
    spaced grid. You have to use Lua scripting to do it, but it's not
    that big a deal to do. There is an example at:
    http://groups.yahoo.com/group/femm/files/scripting/grid.zip
    that might be helpful.

    Dave.

- Follow-Ups:
  - reading out data with lua grid script
    - From: "eborkent" <eborkent@yahoo.com>

- References:
  - Re: permanent magnet in harmonic analysis
    - From: E-J Borkent <eborkent@yahoo.com>

- Prev by Date: Re: permanent magnet in harmonic analysis
- Next by Date: file name update
- Previous by thread: Re: permanent magnet in harmonic analysis
- Next by thread: reading out data with lua grid script
- Index(es):
  - Date
  - Thread