[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Re: [femm] Total current in a high energy disharge.

- To: femm@yahoogroups.com
- Subject: Re: [femm] Total current in a high energy disharge.
- From: Dave Squires <djsquires@plix.com>
- Date: Mon, 16 Apr 2001 16:49:09 -0700
- References: <8f.963106d.280cc605@aol.com>

    fucian@aol.com wrote:

    > Ok, I was thinking of adding resistance to lower current draw.Im fully aware
    > of the dangers.I dont fool around like you may think.

    Well, that's good. You never know.

    > One thing is I need to
    > know the type of resistor to use as a bleeder.I know I need like a 10K 50
    > watt or so but what TYPE is good?Im thinking metal oxide?

    Well, a non-inductive one. 10K seems high. What peak current
    do you need? Just use Ohm's Law to figure R.

    Dave Squires

    > Matt
    >
    >
    >
    > Your use of Yahoo! Groups is subject to http://docs.yahoo.com/info/terms/

- References:
  - Re: [femm] Total current in a high energy disharge.
    - From: fucian@aol.com

- Prev by Date: Re: [femm] Total current in a high energy disharge.
- Next by Date: Re: [femm] Total current in a high energy disharge.
- Previous by thread: Re: [femm] Total current in a high energy disharge.
- Next by thread: Re: Total current in a high energy disharge.
- Index(es):
  - Date
  - Thread